RCA report for LX-70

Motor cutoff observed with battery No. 02 (V2)

**Issue Number:** LX70-I278

**Data Link:** [https://cloud.bytebeam.io/projects/lectrix/dashboards/653?id=4&timeRange=%7B%22type%22%3A%22AbsoluteTimeRange%22%2C%22from%22%3A%7B%22type%22%3A%22AbsoluteTimestamp%22%2C%22date%22%3A1710381600000%7D%2C%22to%22%3A%7B%22type%22%3A%22AbsoluteTimestamp%22%2C%22date%22%3A1710383426000%7D%7D](https://cloud.bytebeam.io/projects/lectrix/dashboards/653?id=4&timeRange={"type"%3A"AbsoluteTimeRange"%2C"from"%3A{"type"%3A"AbsoluteTimestamp"%2C"date"%3A1710381600000}%2C"to"%3A{"type"%3A"AbsoluteTimestamp"%2C"date"%3A1710383426000}})

**Description:**

**Date:** 14-03-2024

**Time:** 7:47 AM

**Vehicle No:** V2

**Byte beam No:** 04

**Battery No:** 02

**Mode:** Custom before 7:43Am, Power at cutoff

**Analysis:**

**Cause 1:** undervoltage

**Cause 2:** Custom mode (should be not be used for testing)

Solution : use other mode (ECO and Sports) not custom